**PORTABLE DIGITAL METERS**

**TLC-DM1**

 For the measurement of:200mA/2mA/20mA/200mA/2A/20A, ANY SINGLE RANGE

 Bench Top main operated

 7 segment LED type of 20/30mm(H) 3½ digit digital display

 1 in +1999 resolution for all measurements

 Accuracy less than +0.5%, for +2 least counts

**TLC-DM2**

 For the measurement of:200mV/2V/20V/200V/2000V, ANY SINGLE RANGE

 Bench Top main operated

 7 segment LED type of 20/30mm(H) 3½ digit digital display

 1 in +1999 resolution for all measurements

 Accuracy +0.1%, for +2 least counts

 Accuracy for 20V-1000V is +0.2%, for +2 least counts

**TLC-DM3**

 For the measurement of:200mA/2mA/20mA/200mA/2A/20A, ANY SINGLE RANGE

 Bench Top main operated

 7 segment LED type of 20/30mm(H) 3½ digit digital display

 1 in +1999 resolution for all measurements

 Accuracy less than +0.5%, for +2 least counts

**TLC-DM4**

 For the measurement of:200mV/2V/20V/200V/2000V ANY SINGLE RANGE

 Bench Top main operated

 7 segment LED type of 20/30mm(H) 3½ digit digital display

 1 in +1999 resolution for all measurements

 Accuracy +0.1%, for +2 least counts

 Accuracy for 20V-1000V is +0.2%, for +2 least counts

**TLC-DM5**

 For the measurement of:200uA/2000mA/200V/200mA/2V/20V

 Bench Top main operated

 7 segment LED type of 20/30mm(H) 3½ digit digital display

 1 in +1999 resolution for all measurements

 Accuracy +0.5%