# DECADE BOXES

**DECADE CAPACITANCE BOXES**

 Special thumbwheel switches

 Polyster capacitors

 Accuracy +1%

 4 Decade - 100PF to 1μF

 5 Decade - 100PF to 10μF

 6 Decade- 100PF to 100Μf

**DECADE INDUCTANCE BOXES**

 Special rotary swiches with low contact resistance

 With fuse protection

 Accuracy +5%

 4 Decade- 10μH to 100mH

  5 Decade - 10μH to 1H

**DECADE RESISTANCE BOXES**

 Special rotary swiches with low contact resistance

 Wire wound resistors for lower values

 Accuracy +1%

 With fuse protection

 4 Decade - 10Ω to 100KΩ

 5 Decade- 10Ω to 1MΩ

 6 Decade- 1Ω to 1MΩ